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[bookmark: _GoBack]The Change heat exchanger gasket is incredibly robust and resilient, and is designed to deliver the most dynamic seal ever. It’s manufactured with proprietary equipment, using a 5-times thicker metal spiral and a unique laser welding process that penetrates completely through. As a result, it requires no inner or outer ring, and is as easy to handle and install as a double-jacketed gasket. Furthermore, it’s proven to perform without fail at least 60% longer than any other heat exchanger gasket, spiral wound, double jacketed, CMG, or Kammprofile. 
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